    // ------------------------------- //
    // -------- Start of File -------- //
    // ------------------------------- //
    // ----------------------------------------------------------- //
    // C++ Header File Name: gxsfile.h
    // C++ Compiler Used: MSVC, BCC32, GCC, HPUX aCC, SOLARIS CC
    // Produced By: DataReel Software Development Team
    // File Creation Date: 09/20/1999
    // Date Last Modified: 06/17/2016
    // Copyright (c) 2001-2024 DataReel Software Development
    // ----------------------------------------------------------- //
    // ---------- Include File Description and Details  ---------- //
    // ----------------------------------------------------------- //
    /*
    This library is free software; you can redistribute it and/or
    modify it under the terms of the GNU Lesser General Public
    License as published by the Free Software Foundation; either
    version 2.1 of the License, or (at your option) any later version.

    This library is distributed in the hope that it will be useful,
    but WITHOUT ANY WARRANTY; without even the implied warranty of
    MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
    Lesser General Public License for more details.

    You should have received a copy of the GNU Lesser General Public
    License along with this library; if not, write to the Free Software
    Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307
    USA

    The gxsFile class is used to move data to and from disk
    files using the device cache.
    */
    // ----------------------------------------------------------- //
    #ifndef __GXS_FILE_HPP__
    #define __GXS_FILE_HPP__

    #include "gxdlcode.h"

    #include <stdlib.h>
    #include "devcache.h"
    #include "membuf.h"
    #include "memblock.h"
    #include "gxstream.h"
    #include "gxdatagm.h"
    #include "scomserv.h"
    #include "dfileb.h"

    class gxsFile : public gxDeviceCache
    {
    public:
      gxsFile(int CacheSize = 1024);
      ~gxsFile() { }

    public:
      void DeviceErrorHandler(const char *mesg);
      void Flush(); // Flush the cache buckets to the output device
      unsigned BucketsInUse() { return cache.BucketsInUse(); }
      void CloseOutputFile();
      void CloseInputFile();
      int OpenInputFile(const char *in);
      int OpenOutputFile(const char *out);
      FAU_t LoadFile(gxDeviceCachePtr p, FAU_t end_of_file);
      int CopyFileToFile(FAU_t &byte_count);
      int CopyFileToStreamSocket(gxStream *s, FAU_t &byte_count);
      int CopyFileToDatagramSocket(gxDatagram *s, FAU_t &byte_count);
      int CopyFileToSerialPort(gxSerialCommServer *s, FAU_t &byte_count);
      int CopyStreamSocketToFile(gxStream *s, gxBlockHeader &gxs);
      int CopyDatagramSocketToFile(gxDatagram *s, gxBlockHeader &gxs);
      int CopySerialPortToFile(gxSerialCommServer *s, gxBlockHeader &gxs);

    private: // Base class interface
      void Read(void *buf, unsigned Bytes, gxDeviceTypes dev);
      void Write(const void *buf, unsigned Bytes, gxDeviceTypes dev);

    private: // Device objects
      DiskFileB outfile;               // File used to output data
      DiskFileB infile;                // File used to input data
      gxStream *stream_sock;           // Stream socket (network device)
      gxDatagram *datagram_sock;       // Datagram socket (network device)
      gxSerialCommServer *serial_port; // Serial port (RS232 device)

    private: // Temporary variables used during read/write operations
      gxBlockHeader curr_stream_hdr;
      gxBlockHeader curr_datagram_hdr;
      gxBlockHeader curr_serial_hdr;

    private: // Device cache
      gxDeviceBucketCache cache;

    public: // Functions used to get the current device cache
      gxDeviceBucketCache *GetCache() { return &cache; }
    };

    #endif // __GXS_FILE_HPP__
    // ----------------------------------------------------------- //
    // ------------------------------- //
    // --------- End of File --------- //
    // ------------------------------- //